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	Notsi Solar Park (475 MW) Request for Quotation (RFQ)
	Doc No.
	NSI-00-PR-QUO-001

	
	
	Rev. No.
	00

	
	
	Rev. Date
	05/05/2026






	Date:
	15 May 2026
	
	RFQ Reference Number:
	CNWE-SH-RFQ-2026-024




You are hereby invited to tender for the below mentioned Scope of Work / Supply, in accordance with the Project Specifications and Requirements as specified.



	Project Details:
	

	Project Name:
	Notsi 475MW Solar Park

	Contract No:
	

	Location:
	Dealesville, Freestate, Tokologo Municipality

	Completion Date:
	5 May 2028





	RFQ Specific Details:
	

	Scope of Work/Supply:
	The appointed Service Provider shall supply a suitable dust suppression chemical/product for the PV Project.
The product must be suitable for use on construction site roads, internal access roads, laydown areas, disturbed soil areas and other areas where dust control is required.
The product must support compliance with the project EMPr, Environmental Authorisation, site HSE requirements, environmental requirements, and applicable South African legislation. The supplier must provide a current Safety Data Sheet in line with the Hazardous Chemical Agents Regulations, 2021, where applicable. These Regulations require classification and Safety Data Sheet information for hazardous chemical agents. 
1. Product to be Tendered On
The Service Provider must tender on the supply of dust suppression chemical/product suitable for construction site use.
The quotation must include:
	No.
	Item
	Requirement

	1
	Dust suppression product
	Product suitable for unpaved construction roads and exposed soil areas

	2
	Product specification
	Full product technical data sheet to be provided

	3
	Safety Data Sheet
	Current SDS to be provided

	4
	Environmental information
	Product must not cause soil, groundwater, stormwater or vegetation contamination

	5
	Application method
	Supplier to provide recommended application method

	6
	Dosage rate
	Supplier to provide dilution ratio and application rate

	7
	Demonstration
	Supplier to conduct a product demonstration on site, where required

	8
	Storage requirements
	Supplier to provide safe storage requirements

	9
	Handling requirements
	Supplier to provide safe handling and PPE requirements

	10
	Spill response
	Supplier to provide spill clean-up and emergency response requirements


2. Minimum Product Requirements
The dust suppression product must:
· Be suitable for construction site conditions.
· Be suitable for gravel roads, access roads, laydown areas and disturbed soil surfaces.
· Reduce dust generation from vehicle movement and wind.
· Be safe for use around workers, vehicles, plant and construction equipment.
· Be compatible with water-based application methods, where applicable.
· Not create unsafe slippery road conditions when applied correctly.
· Not damage vehicles, plant, tyres or equipment.
· Not cause unacceptable soil or water pollution.
· Not negatively impact surrounding vegetation when used correctly.
· Be supported by a valid technical data sheet and SDS.
· Include clear application instructions.
· Include clear storage and handling requirements.
3. Demonstration Requirement
The Service Provider must allow for a product demonstration on site, where required by the project team.
The demonstration must show:
· Product mixing requirements.
· Application method.
· Recommended dosage rate.
· Expected drying or curing time.
· Expected dust suppression performance.
· Reapplication frequency.
· Any road safety concerns.
· Any environmental precautions.
· Any PPE requirements for handling and application.
4. Documentation Required
The Service Provider must submit the following with the quotation:
· Company profile.
· Product technical data sheet.
· Current Safety Data Sheet.
· Product composition summary, where available.
· Recommended application method.
· Recommended dilution ratio.
· Recommended application rate per square metre or per kilometre.
· Expected reapplication frequency.
· Storage requirements.
· PPE/C requirements.
· Spill response procedure.
· Environmental precautions.
· Confirmation that the product is suitable for construction site use.
· Confirmation that the product is suitable for PV project access roads and exposed soil areas.
· Product test results, case studies or references, where available.
5. Environmental Requirements
The product must be suitable for use in an environmentally controlled construction project.
The Service Provider must confirm that the product will not cause unacceptable pollution or degradation when used according to the supplier’s instructions.
The National Environmental Management Act places a duty of care on persons who cause, have caused, or may cause significant pollution or degradation to take reasonable measures to prevent it. The National Water Act also requires reasonable measures to prevent pollution of water resources where pollution occurs or is likely to occur from activities on land. 
The supplier must provide controls for:
· Protection of soil.
· Protection of stormwater systems.
· Protection of drainage lines.
· Protection of vegetation.
· Spill prevention.
· Safe storage.
· Safe handling.
· Disposal of empty containers.
· Management of unused product.
6. Pricing Requirements
The quotation must clearly show:
· Product name.
· Product unit size.
· Cost per litre, kilogram, drum, IBC or bulk load.
· Minimum order quantity.
· Delivery cost.
· Delivery lead time.
· Cost for site demonstration, if applicable.
· Cost for technical support, if applicable.
· Estimated coverage rate.
· Estimated cost per square metre or kilometre treated.
· VAT.
· Any exclusions.
7. Tender Submission Requirements
The Service Provider must confirm:
· Product availability.
· Delivery timeframe.
· Storage requirements.
· Shelf life.
· Whether the product requires dilution.
· Whether special application equipment is required.
· Whether the supplier provides application equipment.
· Whether the supplier provides application services.
· Whether training or toolbox talk support can be provided.
· Whether the product is hazardous or non-hazardous.
· Whether the product is biodegradable, where applicable.
· Whether empty containers can be collected or returned.
8. Project Requirement
The dust suppression chemical/product must be suitable for use on a PV construction project and must support effective dust control without creating unacceptable health, safety or environmental risks.
All product documents must be suitable for review by the project HSE and Environmental teams before the product is approved for use on site.

	Form of Agreement:
	Service provider

	Validity of Quote:
	30 days

	Delivery:
	 As required

	BOQ:
	N/a

	Specifications:
	 As per scope of work

	Drawings:
	N/a

	RFQ Submission Date:
	Date:      25 May 2026                      Time: 16h00

	Submission of Quote:
	By mail: johan@cggcpower.com
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RFQ Specific Requirements:
Duration of activity: Duration of Project Start date:


Service required:
	Quantity
	Type
	Additional specifications

	       
	
	


	
	
	



Terms & Conditions: As per CNWE service agreement contract.
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CNWE Procurement Process & Requirements:

All RFQ’s to be submitted to CRM Office for processing
Procurement of all services will be based on a commercial basis.
Only contractors & SMME’s which have been fully vetted by CRM will be considered.

	Returnable to be submitted (Check List)

	
Quotation / Proposal Including Cover Letter
	

	BEE Certificate / WBHO Affidavit
	

	Certified copy of roadworthy certificate and licence disc
	

	Certified training certificates/competencies of operators
	

	
Service record of plant
	

	
Tax clearance document
	

	
Proof of insurance and ownership
	

	
Vat Registration
	

	
Letter of Good Standing
	

	
Company registration document
	

	
Proof of Address
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