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	Notsi Solar Park (475 MW) Request for Quotation (RFQ)
	Doc No.
	NSI-00-PR-QUO-001

	
	
	Rev. No.
	00

	
	
	Rev. Date
	05/05/2026






	Date:
	15 April 2026
	
	RFQ Reference Number:
	CNWE-SH-RFQ-2026-25




You are hereby invited to tender for the below mentioned Scope of Work / Supply, in accordance with the Project Specifications and Requirements as specified.



	Project Details:
	

	Project Name:
	Notsi 475MW Solar Park

	Contract No:
	

	Location:
	Dealesville, Freestate, Tokologo Municipality

	Completion Date:
	5 May 2028





	RFQ Specific Details:
	

	Scope of Work/Supply:
	The appointed Service Provider shall supply, deliver, install, inspect, service and maintain fire prevention and firefighting equipment for the PV Project.
The equipment must be suitable for a construction site environment and must support compliance with the OHS Act 85 of 1993, Construction Regulations 2014, General Safety Regulations, applicable SANS requirements, project HSE requirements and site emergency response requirements.
Workplaces must have suitable firefighting equipment placed at strategic locations, and the equipment must be maintained in good working order. 
1. Equipment to be Tendered On
	No.
	Equipment / Service
	Requirement

	1
	Fire extinguishers
	DCP, CO₂, foam and water units where required

	2
	Fire extinguisher stands
	Suitable for construction site use

	3
	Fire extinguisher brackets
	For offices, stores, containers and workshops

	4
	Fire blankets
	For kitchens, hot work areas and first response use

	5
	Fire hose reels
	Where required for fixed facilities

	6
	Fire buckets / sand buckets
	For fuel storage and hot work areas where required

	7
	Fire points
	Complete fire point setup with signage and equipment

	8
	Fire signage
	Fire extinguisher, fire point, emergency exit and no smoking signs

	9
	Flammable storage signage
	For fuel, gas, chemicals and flammable material areas

	10
	Hot work fire prevention equipment
	Fire blanket, extinguisher and spark control equipment

	11
	Gas cylinder fire safety equipment
	Signage, securing chains and storage controls where available

	12
	Inspection tags
	Monthly and service inspection tags

	13
	Servicing of extinguishers
	Service, refill, repair and pressure testing

	14
	Replacement units
	Replacement of damaged, expired or discharged units

	15
	Fire equipment register
	Register of all supplied and serviced equipment


2. Minimum Requirements
The Service Provider must ensure that all fire equipment is:
· Suitable for construction site use.
· Suitable for PV project work areas.
· Supplied new or in approved serviceable condition.
· Correctly selected for the fire risk.
· Clearly labelled and identifiable.
· Installed or positioned at agreed locations.
· Accessible and not obstructed.
· Supplied with inspection tags.
· Supplied with service records.
· Maintained in good working order.
· Replaced where damaged, discharged, expired or defective.
· Serviced by competent persons.
Fire extinguishers and hose reels must be serviced and maintained by competent persons in line with applicable SANS requirements, including SANS 1475 and SANS 10105 where applicable. 
3. Areas to be Covered
The Service Provider must allow for fire prevention equipment for the following areas:
· Site offices.
· Site camp.
· Laydown areas.
· Workshops.
· Stores.
· Chemical storage areas.
· Fuel storage areas.
· Waste storage areas.
· Parking areas.
· Hot work areas.
· Generators.
· Temporary electrical areas.
· Substations and inverter areas where required.
· Ablution areas where required.
· Canteen or kitchen areas where required.
· Mobile plant and vehicles where required.
4. Inspection, Servicing and Maintenance
The Service Provider must tender on:
· Initial supply and placement of equipment.
· Monthly inspections where required.
· Annual servicing.
· Refilling of discharged extinguishers.
· Pressure testing where required.
· Replacement of defective equipment.
· Updating of inspection tags.
· Updating of fire equipment registers.
· Emergency replacement after use or damage.
· Issuing of service certificates.
5. Documentation Required
The Service Provider must submit the following with the quotation:
· Company profile.
· Proof of experience in fire equipment supply and servicing.
· SANS 1475 certificate or relevant approval, where applicable.
· SAQCC Fire registration for technicians, where applicable.
· Product catalogue.
· Product specifications.
· Fire extinguisher types available.
· Proposed fire equipment placement recommendation.
· Service and maintenance procedure.
· Inspection checklist.
· Sample fire equipment register.
· Sample service certificate.
· Delivery timeframe.
· Emergency call-out availability.
A public tender example for fire extinguisher and hose reel maintenance requires tenderers to provide SANS 1475 certificate details and SAQCC technician registration details, which is a useful benchmark for this RFQ. 
6. Pricing Requirements
The quotation must clearly show pricing for:
· DCP fire extinguishers.
· CO₂ fire extinguishers.
· Foam fire extinguishers.
· Water fire extinguishers.
· Fire extinguisher stands.
· Fire extinguisher brackets.
· Fire blankets.
· Fire hose reels, where applicable.
· Fire buckets / sand buckets.
· Fire signage.
· Fire point setup.
· Monthly inspection cost.
· Annual service cost.
· Refill cost.
· Pressure test cost.
· Replacement parts.
· Emergency call-out cost.
· Delivery cost.
· VAT.
· Any exclusions.
7. Required Records After Service
The Service Provider must submit:
· Fire equipment register.
· Inspection checklist.
· Service certificate.
· Refill certificate, where applicable.
· Pressure test record, where applicable.
· Defect report.
· Replacement record.
· Updated equipment list.
· Invoice linked to serviced or supplied equipment.
8. Project Requirement
All fire prevention and firefighting equipment must be suitable for construction site conditions, PV project activities, hot work, fuel storage, chemical storage, temporary offices, laydown areas, plant areas and emergency response requirements.
All equipment and service records must be suitable for audit purposes and for inclusion in the project HSE file.


	Form of Agreement:
	Service provider

	Validity of Quote:
	30 days

	Delivery:
	 As per agreement

	BOQ:
	Pricing per unit

	Specifications:
	 As per scope of work

	Drawings:
	N/a

	RFQ Submission Date:
	Date:       25 May 2026                     Time: 16h00

	Submission of Quote:
	By mail: johan@cggcpower.com
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RFQ Specific Requirements:
Duration of activity: Duration of Project Start date:


Service required:
	Quantity
	Type
	Additional specifications

	       
	
	


	
	
	



Terms & Conditions: As per CNWE service agreement contract.
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CNWE Procurement Process & Requirements:

All RFQ’s to be submitted to CRM Office for processing
Procurement of all services will be based on a commercial basis.
Only contractors & SMME’s which have been fully vetted by CRM will be considered.

	Returnable to be submitted (Check List)

	
Quotation / Proposal Including Cover Letter
	

	BEE Certificate / WBHO Affidavit
	

	Certified copy of roadworthy certificate and licence disc
	

	Certified training certificates/competencies of operators
	

	
Service record of plant
	

	
Tax clearance document
	

	
Proof of insurance and ownership
	

	
Vat Registration
	

	
Letter of Good Standing
	

	
Company registration document
	

	
Proof of Address
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