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	Date:
	15 May 2026
	
	RFQ Reference Number:
	CNWE-SH-RFQ-2026-026




You are hereby invited to tender for the below mentioned Scope of Work / Supply, in accordance with the Project Specifications and Requirements as specified.



	Project Details:
	

	Project Name:
	Notsi 475MW Solar Park

	Contract No:
	

	Location:
	Dealesville, Freestate, Tokologo Municipality

	Completion Date:
	5 May 2028





	RFQ Specific Details:
	

	Scope of Work/Supply:
	The appointed Service Provider shall supply and deliver fuel for the PV Project, including diesel required for construction vehicles, mobile plant, generators, water bowsers, temporary site facilities and other approved project equipment.
The supplier must provide fuel in compliance with applicable South African fuel quality, transport, storage, environmental and safety requirements. The Petroleum Products Act regulates petroleum products in South Africa, and the National Road Traffic Act includes provisions for the transportation of dangerous goods. 
1. Fuel Supply Required
	No.
	Item / Service
	Requirement

	1
	Diesel supply
	Supply of diesel suitable for construction plant, vehicles and generators

	2
	Bulk fuel delivery
	Delivery to the PV Project site as required

	3
	Mobile refuelling
	Refuelling of approved plant and equipment on site where required

	4
	Fuel bowser supply
	Supplier to confirm if bowsers or mobile tanks can be supplied

	5
	Generator fuel supply
	Fuel supply for site generators where required

	6
	Emergency fuel delivery
	Supplier to confirm emergency delivery availability

	7
	Fuel quality documentation
	Fuel quality certificate or product specification to be provided

	8
	Delivery notes
	Delivery records to be submitted for every delivery

	9
	Fuel reconciliation
	Quantity delivered and received must be recorded

	10
	Spill response
	Supplier must provide spill prevention and emergency response controls


2. Minimum Requirements
The Fuel Supplier must ensure that:
· Fuel supplied is suitable for construction plant, vehicles and generators.
· Fuel quality complies with applicable South African petroleum product requirements.
· Deliveries are done by competent drivers.
· Delivery vehicles are suitable and compliant for fuel transport.
· Fuel transport vehicles are marked, placard and equipped as required for dangerous goods transport.
· Refuelling activities are controlled to prevent spills, fire risk and environmental contamination.
· No fuel is discharged into soil, stormwater areas, drainage lines, excavations or unauthorised areas.
· Fuel delivery and dispensing areas are controlled during refuelling.
· Spill kits are available during delivery and refuelling.
· Fire extinguishers are available on delivery vehicles.
· Delivery vehicles comply with site access, traffic and security requirements.
The transport of dangerous goods in South Africa is regulated through the National Road Traffic Act and supporting standards for dangerous goods identification, packaging, vehicles and transport controls. 
3. Site Delivery Requirements
The supplier must confirm:
· Minimum order quantity.
· Delivery lead time.
· Delivery frequency.
· Delivery area coverage.
· Emergency delivery response time.
· Whether delivery can be done during weekends or after hours.
· Whether mobile refuelling can be done at plant work areas.
· Whether fuel bowsers, tanks or dispensing equipment can be supplied.
· Whether the supplier provides calibrated dispensing meters.
· Whether fuel delivery can be tracked per vehicle, plant item or generator.
4. Fuel Storage and Dispensing Requirements
Where the supplier provides storage tanks, bowsers or dispensing equipment, the supplier must confirm that the equipment includes:
· Safe and suitable fuel storage design.
· Bunding or secondary containment where required.
· Lockable dispensing controls.
· Fuel hose and nozzle in good condition.
· Drip tray or spill containment.
· Earthing / bonding controls where applicable.
· Fire extinguisher.
· Fuel signage.
· No smoking signage.
· Spill kit.
· Inspection checklist.
· Maintenance records.
· Safe operating instructions.
SANS 10089 covers safe practices for petroleum storage, pumping, distribution and related installations, including electrical, earthing and bonding systems for flammable and combustible liquid facilities. 
5. Environmental and HSE Requirements
The supplier must comply with all project HSE and environmental requirements, including:
· Site induction.
· PPE requirements.
· Site traffic management rules.
· Speed limits.
· Refuelling control procedure.
· Spill prevention requirements.
· Emergency response requirements.
· Fire prevention requirements.
· Waste and contaminated material handling requirements.
· Immediate reporting of spills, leaks, incidents or unsafe conditions.
The supplier must clean up any spill caused during delivery, transfer or refuelling and must remove contaminated material for legal disposal where applicable.
6. Records Required
The supplier must submit the following records:
· Delivery notes for each delivery.
· Fuel quantity delivered.
· Fuel type and grade.
· Date and time of delivery.
· Vehicle registration number.
· Driver name.
· Receiving person name and signature.
· Fuel quality certificate or product specification, where required.
· Calibration certificate for dispensing meter, where applicable.
· Fuel usage or reconciliation report, where required.
· Spill or incident report, where applicable.
· Emergency delivery record, where applicable.
7. Tender Submission Requirements
The Fuel Supplier must submit the following with the quotation:
· Company profile.
· Proof of fuel supply experience.
· Proof of experience supplying construction, mining, renewable energy or remote projects.
· Fuel product specification.
· Fuel quality certificate or confirmation of fuel standard.
· Delivery vehicle details.
· Driver competency and dangerous goods transport details, where applicable.
· Details of fuel bowsers, tanks or dispensing equipment offered.
· Spill response procedure.
· Emergency delivery procedure.
· Proof of insurance.
· Proposed delivery method.
· Proposed delivery lead time.
· Pricing schedule.
· Assumptions and exclusions.
8. Pricing Requirements
The quotation must clearly show pricing for:
· Diesel price per litre.
· Delivery cost.
· Minimum order quantity.
· Bulk delivery cost.
· Mobile refuelling cost, where applicable.
· Bowser or tank hire cost, where applicable.
· Pump or dispensing equipment cost, where applicable.
· Emergency delivery cost.
· Weekend or after-hours delivery cost.
· Fuel testing cost, where applicable.
· Travel cost.
· VAT.
· Any exclusions.
9. Project Requirement
All fuel supply, delivery, storage and refuelling activities must be suitable for a construction PV project and must support safe operation of construction vehicles, mobile plant, generators and temporary site equipment.

	Form of Agreement:
	Service provider

	Validity of Quote:
	30 days

	Delivery:
	 As per agreement

	BOQ:
	34 000 liters plus per week

	Specifications:
	 As per the scope of work

	Drawings:
	N/a

	RFQ Submission Date:
	Date:   25 May 2026                         Time: 16h00

	Submission of Quote:
	By mail: johan@cggcpower.com
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RFQ Specific Requirements:
Duration of activity: Duration of Project Start date:


Service required:
	Quantity
	Type
	Additional specifications

	       
	
	


	
	
	



Terms & Conditions: As per CNWE service agreement contract.
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CNWE Procurement Process & Requirements:

All RFQ’s to be submitted to CRM Office for processing
Procurement of all services will be based on a commercial basis.
Only contractors & SMME’s which have been fully vetted by CRM will be considered.

	Returnable to be submitted (Check List)

	
Quotation / Proposal Including Cover Letter
	

	BEE Certificate / WBHO Affidavit
	

	Certified copy of roadworthy certificate and licence disc
	

	Certified training certificates/competencies of operators
	

	
Service record of plant
	

	
Tax clearance document
	

	
Proof of insurance and ownership
	

	
Vat Registration
	

	
Letter of Good Standing
	

	
Company registration document
	

	
Proof of Address
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