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	Notsi Solar Park (475 MW) Request for Quotation (RFQ)
	Doc No.
	NSI-00-PR-QUO-001

	
	
	Rev. No.
	01

	
	
	Rev. Date
	05/05/2026






	Date:
	15 May 2026
	
	RFQ Reference Number:
	CNWE-SH-RFQ-2026-022




You are hereby invited to tender for the below mentioned Scope of Work / Supply, in accordance with the Project Specifications and Requirements as specified.



	Project Details:
	

	Project Name:
	Notsi 475MW Solar Park

	Project Contract No:
	050746

	Location:
	Dealesville, Freestate, Tokologo Municipality

	Completion Date:
	5 May 2028





	RFQ Specific Details:
	

	Scope of Work/Supply:
	Supply of mobile toilets (Rental) and services

	Form of Agreement:
	Service provider

	Validity of Quote:
	14 days

	Delivery:
	 June 2026

	BOQ:
	As per agreement

	Specifications:
	 See below

	Drawings:
	N/a

	RFQ Submission Date:
	Date:    25 May 2026                        Time: 16h00

	Submission of Quote:
	By mail: johan@cggcpower.com
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RFQ Specific Requirements:
Duration of activity: Duration of Project Start date: June 2026


Service required:
	Quantity
	Type
	Additional specifications

	       As per request.
	SUPPLY, SERVICING, MAINTENANCE AND WASTE REMOVAL OF MOBILE TOILET TRAILERS
	
The appointed Service Provider shall supply, deliver, install, service, clean, maintain and remove portable toilets / ablution facilities, empty of 16 000 lt septic tanks weekly for the PV Project.
The service provider must tender on the provision of suitable ablution facilities for a construction site environment, including all labour, transport, servicing, chemicals, consumables, waste removal and disposal requirements.
2. SCOPE OF SERVICES
The appointed Service Provider shall:
· Supply Agri Unit Trailer Ablution Facilities; 
· Deliver units to site; 
· Position and stabilize units safely; 
· Service and cleaning units; 
· Remove sewage and waste; 
· Supply consumables; 
· Maintain and repair units; 
· Provide emergency servicing; 
· Remove units at project completion; and 
· Dispose of waste legally at approved disposal facilities. 

The Service Provider shall include all:
· labour, transport, operators, consumables, chemicals, waste removal, disposal costs, maintenance, PPE, tools, and operational requirements necessary for full-service delivery. 
3. AGRI UNIT TRAILER SPECIFICATION REQUIREMENTS
All Agri Unit Trailers supplied must comply with the following minimum specifications and operational requirements for construction, mining, agricultural, renewable energy and remote site operations.
3.1 DOUBLE UNIT SPECIFICATIONS
Trailer Construction
· Galvanized chassis construction. 
· Heavy-duty mobile trailer design suitable for harsh terrain and site conditions. 
Insulation and Structure
· 40mm Cromadek cold room panels with aluminium sections. 
Weight
· Tare Weight: 550kg 
· Gross Vehicle Mass (GVM): 750kg 
Dimensions
· Cabin Dimensions: 
· 1885mm (L) × 1195mm (W) × 1945mm (H) 
· Overall, Trailer Dimensions: 
· 3270mm (L) × 1595mm (W) × 2485mm (H) 
Suspension and Wheels
· Single axle suspension system. 
· 13-inch wheel size. 
Tank Capacities
· Fresh Water Tank Capacity: 100 litres 
· Waste Tank Capacity: 280 litres 
Standard Components
· Two (2) toilet cubicles. 
· Two (2) wash basins with closable taps. 
· Two (2) toilet paper dispensers. 
· Stabiliser system equalling 4 x Stabilisers. 
· Chemical flush system. 
3.2 STANDARD FEATURES
Each Agri Unit Trailer must include the following minimum features:
· Hand wash basin with fresh water supply. 
· Separate 100L water tank dedicated to wash basins. 
· Lockable Toilet roll holders. 
· Lockable Hand wash soap dispensers. 
· Lockable Paper towel dispensers. 
· Sanitary bins in female cubicles. 
· Weekly sanitary waste removal and disposal service. 
· Fresh sanitary bin bags supplied during each service. 
· Lockable Soap dispensers with 500ml sachet refills monthly. 
· Indoor and outdoor LED solar lighting for visibility and safety. 
· Durable toilet bowls. 
· Ventilated cubicles. 
· Foot pump flushing mechanism. 
· Spacious and user-friendly layout. 
· Easy-access steps. 
· Fully mobile design for relocation to alternative work areas. 
· 280-litre septic tank integrated into unit base. 

3.3 BRAKING SYSTEM
· The trailer has a GVM of 750kg and a tare weight of 550kg. 
· No braking system is required for this trailer specification in accordance with applicable transport regulations. 

3.4 GENERAL REQUIREMENTS
All units supplied must comply with the following minimum requirements:
· Fully licensed and insured units. 
· Pre-shift inspection book to be provided with each unit.  
· Lockable toilet paper holders. 
· Additional indicator lights at the top rear of the unit. 
· Indicator bolts enabling doors to be locked from inside. 
· Seat sanitiser dispenser. 
· One LED light inside each cubicle & One LED light externally mounted. 
· Nylocks and HT bolts on leaf springs and axle torqued to 60NM. 
· Nylocks and HT bolts on coupler torqued to 100NM. 
· Wheel nuts torqued to 140NM. 

3.5  WHEEL SAFETY FEATURES
Each unit must include:
A. Chock Blocks
· Heavy-duty wheel chock blocks. 
B. Tyres, Rims, Nuts/Studs and Threads
· Mining-compliant wheel assemblies and fastening systems. 
C. Wheel Nut Indicators
· Visual wheel nut indicators for inspection and safety monitoring. 

3.6 CHASSIS SAFETY FEATURES
Each unit must include:
A. Rear Stand
· Stabilising rear support stand. 
B. Front Stand
· Stabilising front support stand. 
C. Hitch Point Safety Catch
· Secure hitch locking safety catch. 
D. Secondary Connecting Device
· Secondary safety chain or connecting device. 
3.7 VISIBILITY SAFETY FEATURES
A. Indicator Lights
· Functional road and safety indicator lights. 
B. Reflector Tape
· High-visibility reflective tape. 
C. Reflective Triangles
· Reflective triangles replacing traditional chevron boards where applicable. 
D. LED Brake Lights and Taillights
· Rear LED brake and tail lighting systems. 
E. White Reflector Tape
· Additional white reflective safety tape. 
F. Solar LED Beacon Lights
· Solar-powered LED beacon lights installed on all four corners of the unit to improve visibility and safety in mining and low-light environments. 

3.8 SPECIAL EXTERIOR SAFETY FEATURES
A. Insect Prevention Mesh
· Added mesh above doors to prevent bees and insects entering the cubicles. 
B. Snake Prevention Seals
· Closed gaps underneath doors to reduce snake and pest entry. 
C. Protected Air Vent Covers
· Air vents fitted with covers to prevent insects and bees entering the units. 
D. Four Stabiliser System
· Four stabilisers fitted for improved stability on uneven terrain and harsh conditions. 
E. Reflective Safety Markings
· High-visibility reflective strips suitable for mines and low-light conditions. 
F. Reflective Identification Plates
· Reflective ID plates for site tracking and safety identification. Top of FormBottom of Form

4. REQUIRED SERVICES
	No.
	Required Service
	Requirement

	1
	Supply of Agri Unit Trailers
	Suitable for construction sites.

	2
	Delivery to Site
	Delivery to approved work areas

	3
	Positioning and Installation
	Safe placement and stabilisation

	4
	Cleaning and Servicing
	Regular weekly cleaning and sanitising

	5
	Waste Removal
	Safe sewage and waste extraction

	6
	Consumables
	Toilet Paper, soap, sanitiser, chemicals

	7
	Maintenance
	Repairs and replacement of defective components

	8
	Emergency Call-Out
	Additional servicing when required

	9
	Relocation
	Relocation of units as instructed

	10
	Final Removal
	Removal from site at project completion

	11
	Disposal Records
	Legal disposal documentation



5. SERVICING REQUIREMENTS
The Service Provider must ensure that all units are:
· cleaned and sanitised regularly(min of TWICE a week); 
· hygienic and operational; 
· fully stocked with consumables; 
· chemically treated; 
· free from leaks and odours; 
· structurally safe; 
· stabilised against wind and terrain movement; 
· serviced without causing environmental contamination; and 
· repaired or replaced when damaged. 
Additional servicing shall be provided when units become:
· full, unhygienic, unsuitable for use, or overloaded due to site conditions. 
6. WASTE REMOVAL AND DISPOSAL
The Service Provider shall:
· safely remove sewage and waste; 
· transport waste using compliant equipment preferably steal tanks with vacuum pumps; 
· dispose of waste at authorised disposal facilities only; and 
· comply with all environmental legislation. 
Under no circumstances may waste be:
· dumped, 
· buried, 
· discharged, 
· spilled, 
· disposed into stormwater systems, 
· or disposed at unauthorised locations. 
The Service Provider must provide:
· disposal certificates, 
· and proof of lawful disposal. 

7. SITE COMPLIANCE REQUIREMENTS
The Service Provider must comply with all project site rules including:
· site induction requirements; 
· access control procedures; 
· PPE requirements; 
· vehicle safety standards; 
· environmental controls; 
· speed limits; 
· incident reporting procedures; and 
· spill management requirements. 
All spills, leaks or contamination incidents must be reported immediately and cleaned at the Service Provider’s cost.
8. MINIMUM SUBMISSION REQUIREMENTS
The quotation submission must include:
· Company profile; 
· Proof of experience; 
· Unit specifications; 
· Number of available units; 
· Vehicle fleet details; 
· Operator and driver details; 
· Waste disposal method; 
· Disposal facility information; 
· Servicing frequency proposal; 
· Emergency response capability; 
· Pricing schedule; 
· VAT details; 
· Safety documentation; 
· Proof of legal waste disposal capability; 
· Assumptions and exclusions. 

9. PRICING REQUIREMENTS
Pricing must separately indicate:
· Monthly hire cost per unit; 
· Delivery & Collection cost; 
· Weekly servicing cost; 
· Additional servicing cost; 
· Emergency call-out cost; 
· Waste disposal cost; 
· Relocation cost; 
· Maintenance cost; 
· Consumables cost; 
· VAT. 
10. HEALTH, SAFETY AND ENVIRONMENTAL COMPLIANCE
The Service Provider shall comply with:
· Occupational Health and Safety Act; 
· National Environmental Management Act; 
· Waste Management Regulations; 
· Site HSE requirements; 
· Mine Health and Safety requirements (where applicable); 
· all applicable South African legislation. 

11. RECORDS REQUIRED
The Service Provider must maintain and submit:
· Delivery notes; 
· Service registers; 
· Cleaning registers; 
· Waste removal records; 
· Disposal certificates; 
· Maintenance records; 
· Vehicle inspection records; 
· Emergency call-out records; 
· Incident reports; 
· Final removal confirmation. 

12. GENERAL REQUIREMENT
All Agri Unit Trailer facilities supplied must be suitable for:
· harsh terrain, 
· renewable energy projects, 
· agricultural operations, 
· and remote construction site conditions, 
while maintaining hygienic and safe ablution facilities for all personnel and vis
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CNWE Procurement Process & Requirements:

All RFQ’s to be submitted to CRM Office for processing
Procurement of all services will be based on a commercial basis.
Only contractors & SMME’s which have been fully vetted by CRM will be considered.

	Returnable to be submitted (Check List)

	
Quotation / Proposal Including Cover Letter
	

	BEE Certificate / WBHO Affidavit
	

	Certified copy of roadworthy certificate and licence disc
	

	Certified training certificates/competencies of operators
	

	
Service record of plant
	

	
Tax clearance document
	

	
Proof of insurance and ownership
	

	
Vat Registration
	

	
Letter of Good Standing
	

	
Company registration document
	

	
Proof of Address
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